**NeonSwitch Configuration Notes**

1. Make sure the following ports are NATed to the server and open for inbound traffic in the Windows Firewall:  
     
   UDP: 16384-32758 (RTP)  
   UDP: 4569 (IAX/IAX2)  
   UDP: 5060 SIP-Internal  
   TCP: 5060 SIP-Internal  
   UDP: 5080 SIP-External  
   TCP: 5080 SIP-External  
   UDP: 8000 MRCP  
   TCP: 8000 MRCP
2. Edit **conf\vars.xml**, adding the server’s external IP address:  
     
   <X-PRE-PROCESS cmd="set" data="external\_rtp\_ip=**ExternalIP**"/>  
   <X-PRE-PROCESS cmd="set" data="external\_sip\_ip=**ExternalIP**"/>
3. Vitelity.com Configuration:  
     
   <http://wiki.freeswitch.org/wiki/Provider_Configuration:_Vitelity>   
   <http://wiki.freeswitch.org/wiki/Connecting_Freeswitch_And_Asterisk> (good info)